# 3GPP Power Saving Mode (PSM)

Only for LE866, To ensure the 3GPP Rel 12 compliance when using the SIM in PSM states, it is suggested to use two latches on the SIM\_RST and SIM\_CLK lines.

The two latches are enabled by the PSM\_STATUS line as indicated in the figure below:




Figure 7‑1 PSM Status